<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<text>retrotronics.org</text>
<text>Rev.P1</text>
<text>+3.3V</text>
<text>TDO</text>
<text>TDI</text>
<text>TCK</text>
<text>TMS</text>
<text>GND</text>
<text>Config Only = ON</text>
<text>Normal Mode = OFF</text>
<text>TX</text>
<text>RX</text>
<text>BOOT1/0</text>
<text>GND</text>
<text>SWDAT</text>
<text>SWCLK</text>
<text>+3V3</text>
<text>NC</text>
<text>NC</text>
</plain>
<libraries>
<library name="alan_common">
<packages>
<package name="OSHW_LOGO">
</package>
<package name="KOA_RNET_8MMBSC_0603">
</package>
<package name="SOT223-T">
<description>SOT223 Tabbed Landing</description>
</package>
<package name="ISSI_54L_400MIL_TSOP-2">
</package>
<package name="HDR_1X6">
</package>
<package name="SST_SOIC-8-S2A">
</package>
<package name="LATTICE_TQFP144">
</package>
<package name="NXP_TSSOP24">
</package>
<package name="SMT_0603">
</package>
<package name="NXP_TSSOP56_NEW">
</package>
<package name="TQFP64_5MM">
</package>
<package name="ABRACON_ASDMB">
</package>
<package name="LUMEX_TRILED">
</package>
<package name="DIP1_SMT">
</package>
<package name="LINX_CR2032_HOLDER">
</package>
<package name="MOLEX_MICROSD">
</package>
<package name="ST_EMIF06">
</package>
<package name="USB-A">
</package>
<package name="HDR_1X2">
</package>
<package name="MSOP-8-EP">
</package>
<package name="HDR_2X17">
</package>
<package name="TSSOP-14">
</package>
<package name="ISA_EMS8">
</package>
<package name="NXP_TSSOP20_65">
</package>
<package name="DIP2_SMT">
</package>
<package name="HDR_2X5">
</package>
<package name="HDR_1X4">
</package>
<package name="NXP_SC88-5">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="alan_common" package="OSHW_LOGO" value="OSHW_LOGO"/>
<element name="U5" library="alan_common" package="ISSI_54L_400MIL_TSOP-2" value="ISSI_42S16160D">
<attribute name="NAME"/>
<attribute name="MANF" value="ISSI"/>
<attribute name="MANF#" value="IS42S16160D-7TL"/>
<attribute name="MOUSER#" value="870-42S16160D-7TL"/>
</element>
<element name="U4" library="alan_common" package="NXP_TSSOP24" value="NXP_CBTD3384">
<attribute name="NAME"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="CBTD3384PW,118"/>
<attribute name="MOUSER#" value="771-CBTD3384PW118"/>
</element>
<element name="VR1" library="alan_common" package="SOT223-T" value="NCP1117">
<attribute name="NAME"/>
</element>
<element name="C1" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="U1" library="alan_common" package="SST_SOIC-8-S2A" value="SST25VF032B">
<attribute name="NAME"/>
</element>
<element name="C12" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
<attribute name="MANF" value="TDK"/>
<attribute name="MANF#" value="C3216X5R0J226K/1.6"/>
<attribute name="MOUSER#" value="810-C3216X5R0J226K-5"/>
</element>
<element name="C2" library="alan_common" package="SMT_0603" value="0">
<attribute name="NAME"/>
</element>
<element name="C4" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C3" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="U3" library="alan_common" package="LATTICE_TQFP144" value="LCMXO2-7000">
<attribute name="NAME"/>
</element>
<element name="RA1" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="RA2" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="RA3" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="RA5" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="RA4" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="C13" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C14" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C15" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C16" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C18" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C20" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C22" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C24" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C27" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C30" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C17" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C19" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C21" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C23" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C25" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="C28" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
</element>
<element name="R3" library="alan_common" package="SMT_0603" value="10K">
<attribute name="NAME"/>
</element>
<element name="R1" library="alan_common" package="SMT_0603" value="10K">
<attribute name="NAME"/>
</element>
<element name="C10" library="resistor" package="C1206" value="47uF">
<attribute name="NAME"/>
</element>
<element name="U2" library="alan_common" package="NXP_TSSOP56_NEW" value="NXP_CBTD16211N">
<attribute name="NAME"/>
</element>
<element name="C7" library="resistor" package="C1206" value="47uF">
<attribute name="NAME"/>
</element>
<element name="SW1" library="alan_common" package="DIP1_SMT" value="DIP1">
<attribute name="MANF#" value="CHS-01TA"/>
<attribute name="MANF" value="Copal"/>
</element>
<element name="U9" library="alan_common" package="TQFP64_5MM" value="STM32F405">
<attribute name="NAME"/>
</element>
<element name="XO2" library="alan_common" package="ABRACON_ASDMB" value="ABRACON_ASDMB"/>
<element name="D2" library="alan_common" package="LUMEX_TRILED" value="LUMEX_LX0404">
<attribute name="NAME"/>
</element>
<element name="XO1" library="alan_common" package="ABRACON_ASDMB" value="ABRACON_ASDMB"/>
<element name="C32" library="alan_common" package="SMT_0603" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C34" library="alan_common" package="SMT_0603" value="4.7nF">
<attribute name="NAME"/>
</element>
<element name="R6" library="alan_common" package="SMT_0603" value="1M">
<attribute name="NAME"/>
</element>
<element name="R2" library="alan_common" package="SMT_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="BAT1" library="alan_common" package="LINX_CR2032_HOLDER" value="LINX_BAT_HLD-001">
<attribute name="MOUSER#" value="712-BAT-HLD-001"/>
<attribute name="MANF#" value="712-BAT-HLD-001"/>
<attribute name="MANF" value="Linx"/>
</element>
<element name="USD" library="alan_common" package="MOLEX_MICROSD" value="MOLEX_MICROSD">
<attribute name="MANF#" value="0473093751"/>
<attribute name="DIGIKEY#" value="WM3974CT-ND"/>
<attribute name="MANF" value="Molex"/>
</element>
<element name="U10" library="alan_common" package="ST_EMIF06" value="ST_EMIF06">
<attribute name="NAME"/>
</element>
<element name="USB2" library="alan_common" package="USB-A" value="USB_STICK_CONNPCB"/>
<element name="PWRSHUNT" library="alan_common" package="HDR_1X2" value="HDR_1X2">
<attribute name="NAME"/>
</element>
<element name="C40" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C39" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C38" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C42" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C43" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="U7" library="alan_common" package="MSOP-8-EP" value="AP2142A">
<attribute name="MOUSER#" value="621-AP2142AMPG-13"/>
<attribute name="MANF#" value="AP2142AMPG-13"/>
<attribute name="MANF" value="Diodes, Inc"/>
<attribute name="NAME"/>
</element>
<element name="C35" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C31" library="alan_common" package="SMT_0603" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C33" library="alan_common" package="SMT_0603" value="4.7nF">
<attribute name="NAME"/>
</element>
<element name="R5" library="alan_common" package="SMT_0603" value="1M">
<attribute name="NAME"/>
</element>
<element name="USB1" library="alan_common" package="USB-A" value="USB_STICK_CONNPCB"/>
<element name="R20" library="alan_common" package="SMT_0603" value="10K">
<attribute name="NAME"/>
</element>
<element name="RESET" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
</element>
<element name="J3" library="alan_common" package="HDR_2X17" value="HDR_2X17">
<attribute name="NAME"/>
</element>
<element name="U13" library="alan_common" package="TSSOP-14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="alan_common" package="TSSOP-14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U12" library="alan_common" package="TSSOP-14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="NAME"/>
</element>
<element name="C45" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="NAME"/>
</element>
<element name="C46" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="NAME"/>
</element>
<element name="R21" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R22" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R23" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R24" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R25" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R26" library="alan_common" package="SMT_0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="alan_common" package="ISA_EMS8" value="ISA_EMS8"/>
<element name="CONSOLE" library="alan_common" package="HDR_1X6" value="HDR_1X6">
<attribute name="NAME"/>
</element>
<element name="RA6" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22"/>
<element name="RA7" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22"/>
<element name="U8" library="alan_common" package="NXP_TSSOP20_65" value="16V8">
<attribute name="NAME"/>
</element>
<element name="SW2" library="alan_common" package="DIP2_SMT" value="DIP2"/>
<element name="R18" library="alan_common" package="SMT_0603" value="47K">
<attribute name="NAME"/>
</element>
<element name="R19" library="alan_common" package="SMT_0603" value="47K">
<attribute name="NAME"/>
</element>
<element name="R14" library="alan_common" package="SMT_0603" value="100">
<attribute name="NAME"/>
</element>
<element name="R15" library="alan_common" package="SMT_0603" value="100">
<attribute name="NAME"/>
</element>
<element name="J1" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;">
<attribute name="NAME"/>
</element>
<element name="RA8" library="alan_common" package="KOA_RNET_8MMBSC_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="J2" library="alan_common" package="HDR_1X4" value="HDR_1X4">
<attribute name="NAME"/>
</element>
<element name="C36" library="alan_common" package="SMT_0603" value="22pF">
<attribute name="NAME"/>
</element>
<element name="U6" library="alan_common" package="NXP_SC88-5" value="74AHCT1G14">
<attribute name="NAME"/>
</element>
<element name="R10" library="alan_common" package="SMT_0603" value="5K">
<attribute name="NAME"/>
</element>
<element name="R12" library="alan_common" package="SMT_0603" value="5K">
<attribute name="NAME"/>
</element>
<element name="R13" library="alan_common" package="SMT_0603" value="5K">
<attribute name="NAME"/>
</element>
<element name="R11" library="alan_common" package="SMT_0603" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R17" library="alan_common" package="SMT_0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R16" library="alan_common" package="SMT_0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R27" library="alan_common" package="SMT_0603" value="22">
<attribute name="NAME"/>
</element>
<element name="C37" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="R7" library="alan_common" package="SMT_0603" value="57">
<attribute name="NAME"/>
</element>
<element name="R8" library="alan_common" package="SMT_0603" value="57">
<attribute name="NAME"/>
</element>
<element name="R9" library="alan_common" package="SMT_0603" value="57">
<attribute name="NAME"/>
</element>
<element name="D1" library="led" package="CHIPLED_0603" value="LED">
<attribute name="MOUSER#" value="638-19217BHCN1P23"/>
<attribute name="MANF#" value="EL-19-217/BHC-AN1P2/3T"/>
<attribute name="MANF" value="Everlight"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="resistor" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="C11" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C41" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="resistor" package="C1206" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C29" library="alan_common" package="SMT_0603" value="2.2pF">
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="NAME"/>
</element>
<element name="C26" library="alan_common" package="SMT_0603" value=".1uF">
<attribute name="MOUSER#" value="80-C0603C104K5R"/>
<attribute name="MANF#" value="C0603C104K5RACTU"/>
<attribute name="MANF" value="Kemet"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U5" pad="54"/>
<contactref element="U5" pad="28"/>
<contactref element="U5" pad="41"/>
<contactref element="U5" pad="46"/>
<contactref element="U5" pad="52"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="12"/>
<contactref element="VR1" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U4" pad="12"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="80"/>
<contactref element="U3" pad="101"/>
<contactref element="U3" pad="90"/>
<contactref element="U3" pad="116"/>
<contactref element="U3" pad="134"/>
<contactref element="U3" pad="124"/>
<contactref element="U3" pad="46"/>
<contactref element="U3" pad="64"/>
<contactref element="U3" pad="53"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="29"/>
<contactref element="U3" pad="18"/>
<contactref element="U4" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="U4" pad="13"/>
<contactref element="C10" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="56"/>
<contactref element="U2" pad="55"/>
<contactref element="U2" pad="19"/>
<contactref element="U2" pad="38"/>
<contactref element="U2" pad="49"/>
<contactref element="C7" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="XO1" pad="2"/>
<contactref element="XO1" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U9" pad="12"/>
<contactref element="U9" pad="18"/>
<contactref element="U9" pad="63"/>
<contactref element="BAT1" pad="-"/>
<contactref element="USB2" pad="GND"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="XO2" pad="2"/>
<contactref element="U7" pad="B"/>
<contactref element="U7" pad="1"/>
<contactref element="USB1" pad="GND"/>
<contactref element="C31" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="RESET" pad="3"/>
<contactref element="U10" pad="GND"/>
<contactref element="USD" pad="6"/>
<contactref element="USD" pad="G1"/>
<contactref element="USD" pad="G2"/>
<contactref element="USD" pad="G4"/>
<contactref element="U10" pad="2"/>
<contactref element="U10" pad="GND"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="33"/>
<contactref element="J3" pad="31"/>
<contactref element="J3" pad="29"/>
<contactref element="J3" pad="27"/>
<contactref element="J3" pad="25"/>
<contactref element="J3" pad="23"/>
<contactref element="J3" pad="21"/>
<contactref element="J3" pad="19"/>
<contactref element="J3" pad="17"/>
<contactref element="J3" pad="15"/>
<contactref element="J3" pad="13"/>
<contactref element="J3" pad="11"/>
<contactref element="J3" pad="9"/>
<contactref element="J3" pad="7"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="3"/>
<contactref element="U12" pad="7"/>
<contactref element="U11" pad="7"/>
<contactref element="U12" pad="7"/>
<contactref element="U11" pad="7"/>
<contactref element="U13" pad="7"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="U8" pad="10"/>
<contactref element="U8" pad="1"/>
<contactref element="U8" pad="11"/>
<contactref element="U8" pad="9"/>
<contactref element="U8" pad="8"/>
<contactref element="U8" pad="7"/>
<contactref element="U8" pad="6"/>
<contactref element="U8" pad="5"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="4"/>
<contactref element="CONSOLE" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="C36" pad="2"/>
<contactref element="U6" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="C37" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C11" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="U$1" pad="B31"/>
<contactref element="U$1" pad="PLATE2"/>
<contactref element="U$1" pad="PLATE1"/>
<contactref element="U$1" pad="B10"/>
<contactref element="U$1" pad="B1"/>
<contactref element="U$1" pad="B31"/>
<contactref element="U$1" pad="PLATE2"/>
<contactref element="U$1" pad="PLATE1"/>
<contactref element="U$1" pad="B10"/>
<contactref element="U$1" pad="B1"/>
</signal>
<signal name="+5V">
<contactref element="U4" pad="24"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="VR1" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="C7" pad="1"/>
<contactref element="PWRSHUNT" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="U8" pad="20"/>
<contactref element="U6" pad="5"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="ISA_D7">
<contactref element="U$1" pad="A2"/>
<contactref element="U2" pad="26"/>
</signal>
<signal name="ISA_D6">
<contactref element="U$1" pad="A3"/>
<contactref element="U2" pad="27"/>
</signal>
<signal name="ISA_D5">
<contactref element="U$1" pad="A4"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="ISA_D4">
<contactref element="U$1" pad="A5"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="ISA_D3">
<contactref element="U$1" pad="A6"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="ISA_D2">
<contactref element="U$1" pad="A7"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="ISA_D1">
<contactref element="U$1" pad="A8"/>
<contactref element="U2" pad="22"/>
</signal>
<signal name="ISA_D0">
<contactref element="U$1" pad="A9"/>
<contactref element="U2" pad="21"/>
</signal>
<signal name="+3V3">
<contactref element="U5" pad="43"/>
<contactref element="U5" pad="49"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="9"/>
<contactref element="U5" pad="14"/>
<contactref element="U5" pad="27"/>
<contactref element="VR1" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="U3" pad="72"/>
<contactref element="U3" pad="66"/>
<contactref element="U3" pad="51"/>
<contactref element="U3" pad="37"/>
<contactref element="U3" pad="144"/>
<contactref element="U3" pad="135"/>
<contactref element="U3" pad="123"/>
<contactref element="U3" pad="118"/>
<contactref element="U3" pad="108"/>
<contactref element="U3" pad="102"/>
<contactref element="U3" pad="88"/>
<contactref element="U3" pad="79"/>
<contactref element="U3" pad="36"/>
<contactref element="U3" pad="30"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="7"/>
<contactref element="C28" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="VR1" pad="TAB"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="XO1" pad="4"/>
<contactref element="XO1" pad="1"/>
<contactref element="U9" pad="13"/>
<contactref element="U9" pad="19"/>
<contactref element="U9" pad="32"/>
<contactref element="U9" pad="48"/>
<contactref element="U9" pad="64"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="XO2" pad="4"/>
<contactref element="R20" pad="2"/>
<contactref element="U10" pad="15"/>
<contactref element="USD" pad="4"/>
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="U12" pad="14"/>
<contactref element="U11" pad="14"/>
<contactref element="U13" pad="14"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="C37" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="C2" pad="1"/>
<contactref element="XO1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="FLASH_MOSI">
<contactref element="U1" pad="5"/>
<contactref element="U3" pad="71"/>
</signal>
<signal name="OSC_33">
<contactref element="U3" pad="105"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="ISA_SA0">
<contactref element="U$1" pad="A31"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="ISA_SA1">
<contactref element="U$1" pad="A30"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="ISA_SA2">
<contactref element="U$1" pad="A29"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="ISA_SA3">
<contactref element="U$1" pad="A28"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="ISA_SA4">
<contactref element="U$1" pad="A27"/>
<contactref element="U4" pad="11"/>
</signal>
<signal name="ISA_SA5">
<contactref element="U$1" pad="A26"/>
<contactref element="U4" pad="22"/>
</signal>
<signal name="ISA_SA6">
<contactref element="U$1" pad="A25"/>
<contactref element="U4" pad="21"/>
</signal>
<signal name="ISA_SA7">
<contactref element="U$1" pad="A24"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="ISA_SA8">
<contactref element="U$1" pad="A23"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="ISA_SA9">
<contactref element="U$1" pad="A22"/>
<contactref element="U4" pad="14"/>
</signal>
<signal name="ISA_SA10">
<contactref element="U$1" pad="A21"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="ISA_SA11">
<contactref element="U$1" pad="A20"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="ISA_SA12">
<contactref element="U$1" pad="A19"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="ISA_SA13">
<contactref element="U$1" pad="A18"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="ISA_SA14">
<contactref element="U$1" pad="A17"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="ISA_SA15">
<contactref element="U$1" pad="A16"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="ISA_SA16">
<contactref element="U$1" pad="A15"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="ISA_SA17">
<contactref element="U$1" pad="A14"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="ISA_SA18">
<contactref element="U$1" pad="A13"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="ISA_SA19">
<contactref element="U$1" pad="A12"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="!ISA_IOR">
<contactref element="U$1" pad="B14"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="!ISA_IOW">
<contactref element="U$1" pad="B13"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="!ISA_SMEMR">
<contactref element="U$1" pad="B12"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="!ISA_SMEMW">
<contactref element="U$1" pad="B11"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="ISA_RDY">
<contactref element="U$1" pad="A10"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="SA19">
<contactref element="U2" pad="42"/>
<contactref element="U3" pad="91"/>
</signal>
<signal name="SA18">
<contactref element="U2" pad="44"/>
<contactref element="U3" pad="87"/>
</signal>
<signal name="!IOW">
<contactref element="U2" pad="43"/>
<contactref element="U3" pad="89"/>
</signal>
<signal name="SA17">
<contactref element="U2" pad="46"/>
<contactref element="U3" pad="85"/>
</signal>
<signal name="!IOR">
<contactref element="U2" pad="45"/>
<contactref element="U3" pad="86"/>
</signal>
<signal name="SA16">
<contactref element="U2" pad="47"/>
<contactref element="U3" pad="84"/>
</signal>
<signal name="SA15">
<contactref element="U2" pad="48"/>
<contactref element="U3" pad="83"/>
</signal>
<signal name="SA14">
<contactref element="U2" pad="50"/>
<contactref element="U3" pad="82"/>
</signal>
<signal name="SA13">
<contactref element="U2" pad="51"/>
<contactref element="U3" pad="81"/>
</signal>
<signal name="SDRAM_D1">
<contactref element="U3" pad="2"/>
<contactref element="RA1" pad="3B"/>
</signal>
<signal name="JTAG_TDO">
<contactref element="U3" pad="137"/>
<contactref element="J1" pad="10"/>
<contactref element="U9" pad="8"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="JTAG_TDI">
<contactref element="U3" pad="136"/>
<contactref element="J1" pad="8"/>
<contactref element="U9" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="JTAG_TCK">
<contactref element="U3" pad="131"/>
<contactref element="J1" pad="6"/>
<contactref element="U9" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="JTAG_TMS">
<contactref element="U3" pad="130"/>
<contactref element="J1" pad="4"/>
<contactref element="U9" pad="4"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SDRAM_A4">
<contactref element="RA5" pad="8B"/>
<contactref element="U3" pad="57"/>
</signal>
<signal name="SDRAM_A5">
<contactref element="RA5" pad="7B"/>
<contactref element="U3" pad="56"/>
</signal>
<signal name="SDRAM_A6">
<contactref element="RA5" pad="6B"/>
<contactref element="U3" pad="55"/>
</signal>
<signal name="SDRAM_A7">
<contactref element="U3" pad="54"/>
<contactref element="RA5" pad="5B"/>
</signal>
<signal name="SDRAM_A8">
<contactref element="U3" pad="52"/>
<contactref element="RA5" pad="4B"/>
</signal>
<signal name="SDRAM_A9">
<contactref element="U3" pad="50"/>
<contactref element="RA5" pad="3B"/>
</signal>
<signal name="SDRAM_A11">
<contactref element="U3" pad="49"/>
<contactref element="RA5" pad="2B"/>
</signal>
<signal name="SDRAM_A12">
<contactref element="U3" pad="48"/>
<contactref element="RA5" pad="1B"/>
</signal>
<signal name="SDRAM_CKE">
<contactref element="U3" pad="47"/>
<contactref element="RA4" pad="8B"/>
</signal>
<signal name="SDRAM_CLK">
<contactref element="U3" pad="43"/>
<contactref element="RA4" pad="7B"/>
</signal>
<signal name="SDRAM_DQMH">
<contactref element="U3" pad="42"/>
<contactref element="RA4" pad="6B"/>
</signal>
<signal name="SDRAM_D8">
<contactref element="U3" pad="41"/>
<contactref element="RA4" pad="5B"/>
</signal>
<signal name="SDRAM_D9">
<contactref element="U3" pad="39"/>
<contactref element="RA4" pad="4B"/>
</signal>
<signal name="SDRAM_D10">
<contactref element="U3" pad="38"/>
<contactref element="RA4" pad="3B"/>
</signal>
<signal name="SA0">
<contactref element="U4" pad="2"/>
<contactref element="U3" pad="59"/>
</signal>
<signal name="SA1">
<contactref element="U3" pad="60"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="SA2">
<contactref element="U3" pad="61"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="SA3">
<contactref element="U3" pad="62"/>
<contactref element="U4" pad="9"/>
</signal>
<signal name="SA4">
<contactref element="U3" pad="63"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="SA5">
<contactref element="U4" pad="23"/>
<contactref element="U3" pad="65"/>
</signal>
<signal name="SA6">
<contactref element="U4" pad="20"/>
<contactref element="U3" pad="67"/>
</signal>
<signal name="SA7">
<contactref element="U4" pad="19"/>
<contactref element="U3" pad="68"/>
</signal>
<signal name="SA8">
<contactref element="U4" pad="16"/>
<contactref element="U3" pad="69"/>
</signal>
<signal name="SA9">
<contactref element="U4" pad="15"/>
<contactref element="U3" pad="70"/>
</signal>
<signal name="D0">
<contactref element="U2" pad="36"/>
<contactref element="U3" pad="96"/>
</signal>
<signal name="D1">
<contactref element="U2" pad="35"/>
<contactref element="U3" pad="97"/>
</signal>
<signal name="D3">
<contactref element="U2" pad="33"/>
<contactref element="U3" pad="99"/>
</signal>
<signal name="D4">
<contactref element="U2" pad="32"/>
<contactref element="U3" pad="100"/>
</signal>
<signal name="D5">
<contactref element="U2" pad="31"/>
<contactref element="U3" pad="103"/>
</signal>
<signal name="D6">
<contactref element="U2" pad="30"/>
<contactref element="U3" pad="104"/>
</signal>
<signal name="D2">
<contactref element="U2" pad="34"/>
<contactref element="U3" pad="98"/>
</signal>
<signal name="D7">
<contactref element="U2" pad="29"/>
<contactref element="U3" pad="106"/>
</signal>
<signal name="SDRAM_D11">
<contactref element="RA4" pad="2B"/>
<contactref element="U3" pad="35"/>
</signal>
<signal name="SDRAM_D12">
<contactref element="RA4" pad="1B"/>
<contactref element="U3" pad="34"/>
</signal>
<signal name="SDRAM_D13">
<contactref element="RA3" pad="6B"/>
<contactref element="U3" pad="31"/>
</signal>
<signal name="SDRAM_D14">
<contactref element="RA3" pad="7B"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="SDRAM_D15">
<contactref element="RA3" pad="8B"/>
<contactref element="U3" pad="33"/>
</signal>
<signal name="SDRAM_A3">
<contactref element="RA3" pad="5B"/>
<contactref element="U3" pad="28"/>
</signal>
<signal name="SDRAM_A2">
<contactref element="RA3" pad="4B"/>
<contactref element="U3" pad="27"/>
</signal>
<signal name="SDRAM_A1">
<contactref element="RA3" pad="3B"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="SDRAM_A0">
<contactref element="RA3" pad="2B"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="SDRAM_A10">
<contactref element="RA3" pad="1B"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="SDRAM_BA1">
<contactref element="RA2" pad="8B"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="SDRAM_BA0">
<contactref element="RA2" pad="7B"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="!SDRAM_CS">
<contactref element="RA2" pad="6B"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="!SDRAM_RAS">
<contactref element="RA2" pad="5B"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="!SDRAM_CAS">
<contactref element="RA2" pad="4B"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="!SDRAM_WE">
<contactref element="RA2" pad="3B"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="SDRAM_DQML">
<contactref element="RA2" pad="2B"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="SDRAM_D7">
<contactref element="RA2" pad="1B"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="SDRAM_D6">
<contactref element="RA1" pad="8B"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="SDRAM_D5">
<contactref element="RA1" pad="7B"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="SDRAM_D4">
<contactref element="RA1" pad="6B"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="SDRAM_D3">
<contactref element="RA1" pad="5B"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="SDRAM_D2">
<contactref element="RA1" pad="4B"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="FLASH_CLK">
<contactref element="U1" pad="6"/>
<contactref element="U3" pad="44"/>
</signal>
<signal name="!FLASH_SS">
<contactref element="U3" pad="40"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="EQ_DQ0">
<contactref element="U5" pad="2"/>
<contactref element="RA1" pad="2A"/>
</signal>
<signal name="SDRAM_D0">
<contactref element="U3" pad="1"/>
<contactref element="RA1" pad="2B"/>
</signal>
<signal name="EQ_DQ1">
<contactref element="U5" pad="4"/>
<contactref element="RA1" pad="3A"/>
</signal>
<signal name="EQ_DQ2">
<contactref element="U5" pad="5"/>
<contactref element="RA1" pad="4A"/>
</signal>
<signal name="EQ_DQ3">
<contactref element="U5" pad="7"/>
<contactref element="RA1" pad="5A"/>
</signal>
<signal name="EQ_DQ4">
<contactref element="U5" pad="8"/>
<contactref element="RA1" pad="6A"/>
</signal>
<signal name="EQ_DQ5">
<contactref element="U5" pad="10"/>
<contactref element="RA1" pad="7A"/>
</signal>
<signal name="EQ_D16">
<contactref element="U5" pad="11"/>
<contactref element="RA1" pad="8A"/>
</signal>
<signal name="EQ_DQ7">
<contactref element="U5" pad="13"/>
<contactref element="RA2" pad="1A"/>
</signal>
<signal name="EQ_DQML">
<contactref element="U5" pad="15"/>
<contactref element="RA2" pad="2A"/>
</signal>
<signal name="EQ_WE">
<contactref element="U5" pad="16"/>
<contactref element="RA2" pad="3A"/>
</signal>
<signal name="EQ_CAS">
<contactref element="U5" pad="17"/>
<contactref element="RA2" pad="4A"/>
</signal>
<signal name="EQ_RAS">
<contactref element="U5" pad="18"/>
<contactref element="RA2" pad="5A"/>
</signal>
<signal name="EQ_CS">
<contactref element="U5" pad="19"/>
<contactref element="RA2" pad="6A"/>
</signal>
<signal name="EQ_BA0">
<contactref element="U5" pad="20"/>
<contactref element="RA2" pad="7A"/>
</signal>
<signal name="EQ_BA1">
<contactref element="U5" pad="21"/>
<contactref element="RA2" pad="8A"/>
</signal>
<signal name="EQ_A10">
<contactref element="U5" pad="22"/>
<contactref element="RA3" pad="1A"/>
</signal>
<signal name="EQ_A0">
<contactref element="U5" pad="23"/>
<contactref element="RA3" pad="2A"/>
</signal>
<signal name="EQ_A1">
<contactref element="U5" pad="24"/>
<contactref element="RA3" pad="3A"/>
</signal>
<signal name="EQ_A2">
<contactref element="U5" pad="25"/>
<contactref element="RA3" pad="4A"/>
</signal>
<signal name="EQ_A3">
<contactref element="U5" pad="26"/>
<contactref element="RA3" pad="5A"/>
</signal>
<signal name="EQ_DQ12">
<contactref element="RA4" pad="1A"/>
<contactref element="U5" pad="48"/>
</signal>
<signal name="EQ_DQ11">
<contactref element="RA4" pad="2A"/>
<contactref element="U5" pad="47"/>
</signal>
<signal name="EQ_DQ10">
<contactref element="RA4" pad="3A"/>
<contactref element="U5" pad="45"/>
</signal>
<signal name="EQ_DQ9">
<contactref element="RA4" pad="4A"/>
<contactref element="U5" pad="44"/>
</signal>
<signal name="EQ_DQ8">
<contactref element="RA4" pad="5A"/>
<contactref element="U5" pad="42"/>
</signal>
<signal name="EQ_DQMH">
<contactref element="RA4" pad="6A"/>
<contactref element="U5" pad="39"/>
</signal>
<signal name="EQ_CLK">
<contactref element="RA4" pad="7A"/>
<contactref element="U5" pad="38"/>
</signal>
<signal name="EQ_CKE">
<contactref element="U5" pad="37"/>
<contactref element="RA4" pad="8A"/>
</signal>
<signal name="EQ_A12">
<contactref element="U5" pad="36"/>
<contactref element="RA5" pad="1A"/>
</signal>
<signal name="EQ_A11">
<contactref element="U5" pad="35"/>
<contactref element="RA5" pad="2A"/>
</signal>
<signal name="EQ_A9">
<contactref element="U5" pad="34"/>
<contactref element="RA5" pad="3A"/>
</signal>
<signal name="EQ_A8">
<contactref element="U5" pad="33"/>
<contactref element="RA5" pad="4A"/>
</signal>
<signal name="EQ_A7">
<contactref element="U5" pad="32"/>
<contactref element="RA5" pad="5A"/>
</signal>
<signal name="EQ_A6">
<contactref element="U5" pad="31"/>
<contactref element="RA5" pad="6A"/>
</signal>
<signal name="EQ_A5">
<contactref element="U5" pad="30"/>
<contactref element="RA5" pad="7A"/>
</signal>
<signal name="EQ_A4">
<contactref element="U5" pad="29"/>
<contactref element="RA5" pad="8A"/>
</signal>
<signal name="EA_D13">
<contactref element="RA3" pad="6A"/>
<contactref element="U5" pad="50"/>
</signal>
<signal name="EA_D14">
<contactref element="RA3" pad="7A"/>
<contactref element="U5" pad="51"/>
</signal>
<signal name="EQ_D15">
<contactref element="RA3" pad="8A"/>
<contactref element="U5" pad="53"/>
</signal>
<signal name="FLASH_MISO">
<contactref element="U3" pad="45"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="!OP_ENABLE">
<contactref element="U3" pad="58"/>
<contactref element="R3" pad="1"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="ISA_IRQ7">
<contactref element="U$1" pad="B21"/>
<contactref element="U8" pad="18"/>
</signal>
<signal name="ISA_IRQ5">
<contactref element="U$1" pad="B23"/>
<contactref element="U8" pad="16"/>
</signal>
<signal name="ISA_AEN">
<contactref element="U$1" pad="A11"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="AEN">
<contactref element="U2" pad="40"/>
<contactref element="U3" pad="93"/>
</signal>
<signal name="IRQSEL0">
<contactref element="U3" pad="75"/>
<contactref element="U8" pad="2"/>
</signal>
<signal name="IRQSEL1">
<contactref element="U3" pad="74"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="IRQSEL2">
<contactref element="U3" pad="73"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="USB1_VBUS">
<contactref element="C32" pad="1"/>
<contactref element="USB2" pad="VBUS"/>
<contactref element="U7" pad="7"/>
<contactref element="U9" pad="34"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="C34" pad="1"/>
<contactref element="USB2" pad="S1"/>
<contactref element="USB2" pad="S2"/>
</signal>
<signal name="JTRST">
<contactref element="U9" pad="56"/>
</signal>
<signal name="SPI_CLK">
<contactref element="U9" pad="55"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="BOOT1">
<contactref element="U9" pad="28"/>
<contactref element="R19" pad="2"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="SWCLK">
<contactref element="U9" pad="49"/>
<contactref element="J2" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="U9" pad="46"/>
<contactref element="J2" pad="3"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U9" pad="23"/>
<contactref element="RA6" pad="8B"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U9" pad="22"/>
<contactref element="RA6" pad="7B"/>
</signal>
<signal name="!SPI_SS">
<contactref element="U9" pad="20"/>
<contactref element="RA6" pad="5B"/>
</signal>
<signal name="UART4_RX">
<contactref element="U9" pad="15"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="UART4_TX">
<contactref element="U9" pad="14"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="!SPI_IRQ">
<contactref element="U9" pad="21"/>
<contactref element="RA6" pad="6B"/>
</signal>
<signal name="SDIO_D0">
<contactref element="U9" pad="39"/>
<contactref element="U10" pad="7"/>
</signal>
<signal name="SDIO_D1">
<contactref element="U9" pad="40"/>
<contactref element="U10" pad="8"/>
</signal>
<signal name="SDIO_D2">
<contactref element="U9" pad="51"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="SDIO_D3">
<contactref element="U9" pad="52"/>
<contactref element="U10" pad="4"/>
</signal>
<signal name="SDIO_CLK">
<contactref element="U9" pad="53"/>
<contactref element="U10" pad="6"/>
</signal>
<signal name="SDIO_CMD">
<contactref element="U9" pad="54"/>
<contactref element="U10" pad="5"/>
</signal>
<signal name="MCU_CLK">
<contactref element="U9" pad="5"/>
<contactref element="XO2" pad="3"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="!MCU_RESET">
<contactref element="U9" pad="7"/>
<contactref element="R20" pad="1"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="BOOT0">
<contactref element="U9" pad="60"/>
<contactref element="R18" pad="2"/>
<contactref element="SW2" pad="3"/>
</signal>
<signal name="VBAT_+">
<contactref element="BAT1" pad="+"/>
<contactref element="U9" pad="1"/>
<contactref element="BAT1" pad="P2"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="C33" pad="1"/>
<contactref element="USB1" pad="S1"/>
<contactref element="USB1" pad="S2"/>
</signal>
<signal name="N$8">
<contactref element="U10" pad="11"/>
<contactref element="USD" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="U10" pad="12"/>
<contactref element="USD" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U10" pad="10"/>
<contactref element="USD" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="U10" pad="9"/>
<contactref element="USD" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="U10" pad="14"/>
<contactref element="USD" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U10" pad="13"/>
<contactref element="USD" pad="2"/>
</signal>
<signal name="ISA_5V">
<contactref element="PWRSHUNT" pad="2"/>
<contactref element="U$1" pad="B3"/>
</signal>
<signal name="N$23">
<contactref element="U9" pad="31"/>
<contactref element="C43" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U9" pad="47"/>
<contactref element="C42" pad="1"/>
</signal>
<signal name="USB1_EN">
<contactref element="U7" pad="3"/>
<contactref element="U9" pad="33"/>
</signal>
<signal name="USB0_VBUS">
<contactref element="U9" pad="42"/>
<contactref element="C31" pad="1"/>
<contactref element="USB1" pad="VBUS"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="USB0_DM">
<contactref element="U9" pad="44"/>
<contactref element="USB1" pad="D-"/>
</signal>
<signal name="USB0_DP">
<contactref element="U9" pad="45"/>
<contactref element="USB1" pad="D+"/>
</signal>
<signal name="USB1_DM">
<contactref element="USB2" pad="D-"/>
<contactref element="U9" pad="35"/>
</signal>
<signal name="USB1_DP">
<contactref element="USB2" pad="D+"/>
<contactref element="U9" pad="36"/>
</signal>
<signal name="FD_RY_DCHG">
<contactref element="J3" pad="34"/>
<contactref element="U12" pad="5"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="FD_RD_DATA">
<contactref element="J3" pad="30"/>
<contactref element="U12" pad="3"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="FD_WR_PROT">
<contactref element="J3" pad="28"/>
<contactref element="U12" pad="1"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="FD_TRACK0">
<contactref element="J3" pad="26"/>
<contactref element="U12" pad="9"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="FD_INDEX">
<contactref element="J3" pad="8"/>
<contactref element="U12" pad="13"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="FD_DENSITY">
<contactref element="J3" pad="2"/>
<contactref element="U12" pad="11"/>
<contactref element="U11" pad="8"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="FD_SIDESEL">
<contactref element="J3" pad="32"/>
<contactref element="U13" pad="6"/>
</signal>
<signal name="FD_WRGATE">
<contactref element="J3" pad="24"/>
<contactref element="U13" pad="4"/>
</signal>
<signal name="FD_WRDATA">
<contactref element="J3" pad="22"/>
<contactref element="U13" pad="2"/>
</signal>
<signal name="FD_STEP">
<contactref element="J3" pad="20"/>
<contactref element="U13" pad="12"/>
</signal>
<signal name="FD_STEPDIR">
<contactref element="J3" pad="18"/>
<contactref element="U13" pad="10"/>
</signal>
<signal name="FD_MOTEN">
<contactref element="J3" pad="16"/>
<contactref element="U13" pad="8"/>
</signal>
<signal name="FD_DS2">
<contactref element="J3" pad="14"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="FD_DS1">
<contactref element="J3" pad="12"/>
<contactref element="U11" pad="4"/>
</signal>
<signal name="FD_DS0">
<contactref element="J3" pad="10"/>
<contactref element="U11" pad="2"/>
</signal>
<signal name="FD_DS3">
<contactref element="J3" pad="6"/>
<contactref element="U11" pad="12"/>
</signal>
<signal name="FD_IN_USE">
<contactref element="J3" pad="4"/>
<contactref element="U11" pad="10"/>
</signal>
<signal name="N$22">
</signal>
<signal name="FI_RY_DCHG_E">
<contactref element="U12" pad="6"/>
<contactref element="RA8" pad="7A"/>
</signal>
<signal name="FI_RD_DATA_E">
<contactref element="U12" pad="4"/>
<contactref element="RA8" pad="6A"/>
</signal>
<signal name="FI_WR_PROT_E">
<contactref element="U12" pad="2"/>
<contactref element="RA8" pad="5A"/>
</signal>
<signal name="FI_TRACK0_E">
<contactref element="U12" pad="8"/>
<contactref element="RA8" pad="2A"/>
</signal>
<signal name="FI_DENSITY_E">
<contactref element="U12" pad="10"/>
<contactref element="RA8" pad="3A"/>
</signal>
<signal name="FI_INDEX_E">
<contactref element="U12" pad="12"/>
<contactref element="RA8" pad="4A"/>
</signal>
<signal name="N$25">
</signal>
<signal name="FO_IN_USE_E">
<contactref element="U11" pad="13"/>
<contactref element="RA6" pad="2B"/>
</signal>
<signal name="FO_DENSITY_E">
<contactref element="U11" pad="11"/>
<contactref element="RA6" pad="3B"/>
</signal>
<signal name="FO_DS3_E">
<contactref element="U11" pad="9"/>
<contactref element="RA6" pad="4B"/>
</signal>
<signal name="FO_DS0_E">
<contactref element="U11" pad="5"/>
<contactref element="RA7" pad="7B"/>
</signal>
<signal name="FO_DS2_E">
<contactref element="U11" pad="3"/>
<contactref element="RA7" pad="8B"/>
</signal>
<signal name="FO_DS1_E">
<contactref element="U11" pad="1"/>
<contactref element="RA6" pad="1B"/>
</signal>
<signal name="FO_STEP_E">
<contactref element="U13" pad="13"/>
<contactref element="RA7" pad="4B"/>
</signal>
<signal name="FO_STEPDIR_E">
<contactref element="U13" pad="11"/>
<contactref element="RA7" pad="5B"/>
</signal>
<signal name="FO_MOTEN_E">
<contactref element="U13" pad="9"/>
<contactref element="RA7" pad="6B"/>
</signal>
<signal name="FO_SIDESEL_E">
<contactref element="U13" pad="5"/>
<contactref element="RA7" pad="1B"/>
</signal>
<signal name="FO_WRGATE_E">
<contactref element="U13" pad="3"/>
<contactref element="RA7" pad="2B"/>
</signal>
<signal name="FO_WRDATA_E">
<contactref element="U13" pad="1"/>
<contactref element="RA7" pad="3B"/>
</signal>
<signal name="N$26">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="SA10">
<contactref element="U2" pad="54"/>
<contactref element="U3" pad="76"/>
</signal>
<signal name="SA11">
<contactref element="U2" pad="53"/>
<contactref element="U3" pad="77"/>
</signal>
<signal name="SA12">
<contactref element="U2" pad="52"/>
<contactref element="U3" pad="78"/>
</signal>
<signal name="!MEMR">
<contactref element="U2" pad="41"/>
<contactref element="U3" pad="92"/>
</signal>
<signal name="!MEMW">
<contactref element="U2" pad="39"/>
<contactref element="U3" pad="94"/>
</signal>
<signal name="RDY">
<contactref element="U2" pad="37"/>
<contactref element="U3" pad="95"/>
</signal>
<signal name="FO_STEP">
<contactref element="U3" pad="127"/>
<contactref element="RA7" pad="4A"/>
</signal>
<signal name="FO_STEPDIR">
<contactref element="U3" pad="126"/>
<contactref element="RA7" pad="5A"/>
</signal>
<signal name="FO_MOTEN">
<contactref element="U3" pad="125"/>
<contactref element="RA7" pad="6A"/>
</signal>
<signal name="FO_SIDESEL">
<contactref element="U3" pad="133"/>
<contactref element="RA7" pad="1A"/>
</signal>
<signal name="FO_WRGATE">
<contactref element="U3" pad="132"/>
<contactref element="RA7" pad="2A"/>
</signal>
<signal name="FO_WRDATA">
<contactref element="U3" pad="128"/>
<contactref element="RA7" pad="3A"/>
</signal>
<signal name="FO_DS1">
<contactref element="RA6" pad="1A"/>
<contactref element="U3" pad="120"/>
</signal>
<signal name="FO_DS2">
<contactref element="RA7" pad="8A"/>
<contactref element="U3" pad="121"/>
</signal>
<signal name="FO_DS0">
<contactref element="RA7" pad="7A"/>
<contactref element="U3" pad="122"/>
</signal>
<signal name="FO_DS3">
<contactref element="RA6" pad="4A"/>
<contactref element="U3" pad="115"/>
</signal>
<signal name="FO_DENSITY">
<contactref element="RA6" pad="3A"/>
<contactref element="U3" pad="117"/>
</signal>
<signal name="FO_IN_USE">
<contactref element="RA6" pad="2A"/>
<contactref element="U3" pad="119"/>
</signal>
<signal name="ISA_IRQ6">
<contactref element="U$1" pad="B22"/>
<contactref element="U8" pad="17"/>
</signal>
<signal name="ISA_IRQ3">
<contactref element="U$1" pad="B25"/>
<contactref element="U8" pad="12"/>
</signal>
<signal name="ISA_IRQ4">
<contactref element="U$1" pad="B24"/>
<contactref element="U8" pad="13"/>
</signal>
<signal name="ISA_IRQ2">
<contactref element="U$1" pad="B4"/>
<contactref element="U8" pad="19"/>
</signal>
<signal name="ISA_RESET">
<contactref element="U$1" pad="B2"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R15" pad="1"/>
<contactref element="CONSOLE" pad="2"/>
</signal>
<signal name="CON_RTS">
<contactref element="R15" pad="2"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="CON_RX">
<contactref element="CONSOLE" pad="4"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="R14" pad="1"/>
<contactref element="CONSOLE" pad="5"/>
</signal>
<signal name="CON_TX">
<contactref element="R14" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="CON_CTS">
<contactref element="CONSOLE" pad="6"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="FI_RY_DCHG">
<contactref element="U3" pad="143"/>
<contactref element="RA8" pad="7B"/>
</signal>
<signal name="FI_RD_DATA">
<contactref element="U3" pad="142"/>
<contactref element="RA8" pad="6B"/>
</signal>
<signal name="FI_WR_PROT">
<contactref element="U3" pad="141"/>
<contactref element="RA8" pad="5B"/>
</signal>
<signal name="FI_INDEX">
<contactref element="U3" pad="140"/>
<contactref element="RA8" pad="4B"/>
</signal>
<signal name="FI_DENSITY">
<contactref element="U3" pad="139"/>
<contactref element="RA8" pad="3B"/>
</signal>
<signal name="FI_TRACK0">
<contactref element="U3" pad="138"/>
<contactref element="RA8" pad="2B"/>
</signal>
<signal name="SDIO_CD">
<contactref element="U9" pad="57"/>
<contactref element="USD" pad="G3"/>
<contactref element="U10" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="U6" pad="4"/>
<contactref element="U3" pad="107"/>
<contactref element="C29" pad="1"/>
</signal>
<signal name="USB0_EN">
<contactref element="U7" pad="4"/>
<contactref element="U9" pad="43"/>
</signal>
<signal name="SPI_MOSI_PLD">
<contactref element="RA6" pad="8A"/>
<contactref element="U3" pad="110"/>
</signal>
<signal name="SPI_MISO_PLD">
<contactref element="RA6" pad="7A"/>
<contactref element="U3" pad="111"/>
</signal>
<signal name="!SPI_IRQ_PLD">
<contactref element="RA6" pad="6A"/>
<contactref element="U3" pad="113"/>
</signal>
<signal name="!SPI_SS_PLD">
<contactref element="RA6" pad="5A"/>
<contactref element="U3" pad="114"/>
</signal>
<signal name="PLD_LED">
<contactref element="U3" pad="112"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SPI_CLK_PLD">
<contactref element="U3" pad="109"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="!USB0_OC">
<contactref element="U7" pad="5"/>
<contactref element="U9" pad="37"/>
</signal>
<signal name="!USB1_OC">
<contactref element="U9" pad="38"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="LED0">
<contactref element="R7" pad="1"/>
<contactref element="U9" pad="27"/>
</signal>
<signal name="LED1">
<contactref element="R8" pad="1"/>
<contactref element="U9" pad="29"/>
</signal>
<signal name="LED2">
<contactref element="R9" pad="1"/>
<contactref element="U9" pad="30"/>
</signal>
<signal name="N$27">
<contactref element="R9" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R8" pad="2"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="R7" pad="2"/>
<contactref element="D2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
